	Technical specification of H4 mechanical HID set



	●  Imput voltage can be use both 12V and 24V power system。
●   Good  anti-jamming  performance。
●  Double wire hardness circuit，Improving security when driving。
●  8 hours aging&full serial  function testing。


	     Technical specification
characteristic
	H4 mechanical moving

	Imput rated Voltage
	DC12Vdc
（within 11~14Vdc can work normally
	DC24Vdc
（within 22~28Vdc can work normally）

	workelectric current（High beam）
	0.36A（imput12Vdc）
	0.22A(imput 24Vdc）

	Winding resistance
	30Ω
	110Ω

	Winding inductance
	17mH
	57 mH

	Light testing
	Low beam
	Light distribution conform to the ECE R98
	Light distribution conform to the ECE R98

	
	High beam
	Focus lighting
	Focus lighting

	
	High&Low beam  separate (25M)
	≥20cm
	≥20cm

	Continuous moving
	Can be continuous moving 100000 times normally

	Continuous start-up
	Continuous start-up，Mechanical moving can work normally

	condition
	Temperature：－40℃～+105℃，Water-proof&Dust-proof

	spread around hot way
	Working continuously， self-regulation COLD

	Temperature of bulb
	4300K
	5000K
	6000K
	8000K
	10000K
	12000K

	luminous flux
	3200lm
	2900 lm
	2600 lm
	2200 lm
	2000 lm
	1800 lm























